        Itsy V1.5 bill of material
        not including PCB assemblies; includes some accessories


qty/sys	mfgr			P/N		description (on next line)
------------------------------------------------------------------------------

  1	 ---			chassis.prt/.stl
	chassis

  1	 ---			cover.vlm/.dxf/.igs
	front cover

  1	 ---			cursor.sldprt/.stl
	cursor button

 14	North East Fasteners	special
	screw, #2 x5/32", plastic thread, phillips, flat head, Ni-plated steel

  1	Palo Alto Hardware	---
	screw, #4-40 UNC x 1/4"" slotted round-head (for battery box)

  1	Palo Alto Hardware	---
	lockwasher, #4 internal tooth (for battery box)

  1	Palo Alto Hardware	---
	nut, 4-40 UNC (for battery box)

  1	Epson			TCM-A0822-xx
	320x200 reflective LCD display

  1	Dynapro (custom part)	9271 (see NOTE)
	touchscreen (NOTE: must be Rev E or earlier)


I/O/power cable
---------------

  1	Hirose			3240-8P-C
	plug for 8-pin I/O connector

  1	Radio Shack		274-1578 (RSU #10524387)
	barrel-style power jack; 5.5/2.5mm; inline (cord mount)

  1	black stranded hookup wire; approx 1 ft

  1	red/black twisted pair, approx 24AWG; approx 1 ft

  1	shrink wrap for Hirose connector (needed on some assys)

  1	Digital			E116273(UL)CL2
	26AWG DECconnect office cable (6-wire), about 6 ft

  1	Amp			5-555237-1 00
	MMJ connector (modular telephone plug)

  1	electrical tape to prevent shorts in Hirose connector


wall supply
-----------

  1	Radio Shack		273-1666
	wall-mounted regulated supply 800mA, 3/4.5/6VDC (set to 3V)

  1	Switchcraft		760
	5.5/2.5mm power plug

  1	electrical tape to cover voltage select switch


ship kit (including optional items)
-----------------------------------

  1	Itsy motherboard/case assembly

  1	wall supply

  1	I/O/power cable

  1	Digital			H8571-J REV A A
	MMJ (DTE) to DB-9 adapter

  1	McMaster-Carr (dist)	5682A36
	#0 phillips screwdriver; 4.2"-4.4" long, with pocket clip

  1	Pilot Corp		T3200
	stylus/pen (5.6mm OD)

  2	Eveready Energizer	E92 or EN92
	low impedence AAA-size 1.5V alkaline primary cell

  1	Mouser (distributor)	171-3306
	2.5mm stereo plug, hi-rel, shielded (for audio experiments)

  1	 ---			botcover.prt
	optional bottom cover

  1	 ---			battdoor.prt
	battery compartment door for optional bottom cover

  6	Pencom (distributor)
	screw, #2 x 7/32"" plastic thread, phillips, binder head
	(for optional bottom cover)


Copyright (c) Compaq Computer Corporation, 1998, 2000.
For non-commercial use only.  See license agreement.
